Ember+ Standard Parameters

Author: [pbo@l-s-b.de](mailto:pbo@l-s-b.de)  
Date: 2013-02-04  
Revision: 0

The following tree structure contains the definition of standard nodes and parameters Ember+ providers may publish. Implementation of these parameters is optional, unless noted otherwise.

* *Root*
  + **identity**
    - **product**

Syntax: EmberString

Access: Read

*The product name*

* + - **company**

Syntax: EmberString

Access: Read

*String identifying the manufacturing company, optionally including a copyright notice*

* + - **serial**

Syntax: EmberString

Access: Read

*The device serial number in a format defined by the manufacturer; only applicable if the product ships as a hardware unit*

* + - **version**

Syntax: *App defined*

Access: Read

*The provider may publish its version number in any fitting format (usually either EmberString or INTEGER). Only consumers specialized for this provider may interpret this parameter’s value.*

* + - **role**

Syntax:EmberString

Access: Read/Write

*The administrator may set this parameter’s value to any string that identifies the hardware unit. The provider is responsible for keeping this value persistent. This parameter is only applicable if the product ships as a hardware unit.*